Bizmuth — Next SD card image (System/Next 24.11, filesystem-repaired)
====================================================================
This is the official ZX Spectrum Next "System/Next" emulator distribution image
(cspect-next-1gb.img, 24.11) with exactly ONE change:

  The FAT32 filesystem was rebuilt. The upstream image is a malformed FAT32 whose
  cluster count (32,758) falls below the FAT32 minimum (65,525); strict FAT drivers
  — including NextZXOS's esxDOS under pure emulation — cannot create/open files on
  it, so first boot fails with "Error opening 'menu.ini/.def'". We reformatted to a
  spec-correct FAT32 and copied every file back byte-for-byte. Nothing else changed.

Distributed under The Next License (see /LICENSE.md inside the image) — free, in its
entirety, not for sale. NextZXOS/firmware © Garry Lancaster / SpecNext Ltd; the
Spectrum ROMs © Amstrad (redistributed for emulator use per Amstrad's permission).

Also included: tbblue_loader.rom — the Next host bootrom (8KB FPGA loader, Next Core
v3.02.04), part of the Distribution, required to run the Next and not present on the
card itself. Put it in Bizmuth's roms/ folder next to the .img.

Usage: unzip, then drop cspect-next-1gb.img AND tbblue_loader.rom into Bizmuth's roms/ folder
(auto-detected), or pass --sd cspect-next-1gb.img. On first boot pick a video mode (ENTER).
